LFP 13S to 16S CELLS

Analog Front End

BATTERY PACK TERMINAL

CURRENTSENSE

MICROCONTROLLER

Discharge FET

Charge FET

Adaptor input or Load output

Serial Communicn

CAN Interface

Cell Balancing